ReadMe

Fs(accel) = 20000 Hz

AccelC : no leak in flowing water

AccelD : leak in flowing water

Fs(acoustic) = 22050 Hz

AcousticC:  no leak in flowing water

AcousticD:  leak in flowing water